**Installation Instructions**

**IMPORTANT: Read and understand the**

**“General Instructions for Installing SafeTCap**

 **Frame Repair Kits” before you begin.**

1

******

2

Jack up and support the repair side of vehicle leaving the area between tires clear.

**Figure A**

Remove any brackets or line clamps for access to repair area.

******

4

3

******

4

Mark areas to be cut away.

Cut out marked areas and grind surrounding areas clean to prepare for welding.

******

6

5

******

Weld solid all around the new part. Re-attach any brackets that were cut off.

7

8

Coat repair area with paint or undercoating.

Double-check positioning and tack weld in place.

Install new Safe T Cap and clamp in place.

8