
**Installation Instructions**

**IMPORTANT: Read and understand the “General Instructions for Installing SafeTCap Frame Repair Kits” before you begin.**

1. Jack up the front & rear of vehicle and support it on properly rated jack stands. Place rear jack stands under frame, behind rear axle. Make sure the center of vehicle is fully accessible.
2. If you are repairing both sides, **cut & repair one side at a time** keeping one side assembled as a reference/measuring point.

ART-203-R

4

******

3

Mark the centerline of bump stop bracket on upper frame and cut off.

Support rear axle and remove wheel.

******

5

6

8

******

Cut away the rusted area using a plasma cutter, reciprocating saw or torch.

Position the kit into place and roughly mark the outline. Remove kit and grind the frame down to clean metal.

******

8

7

8

******

Slide kit over frame and clamp. Tack weld kit in place. Position bump stop bracket and tack in place. If you are installing additional kits to frame, test-fit those now to make sure they all fit together properly.

Double check all measurements and check door gaps to make sure vehicle stayed straight, then weld all edges 100% solid. If you are adding additional kits, don’t weld the ends yet.

9

******

Prime and paint the repaired area. Use self-tapping screws to remount the brackets that were removed.

**Note:** Numbered pictures in this installation instruction sheet are for demonstration purposes only and may not actually reflect the identical make, model and year of the vehicle you are working on.