
**Installation Instructions**

**IMPORTANT: Read and understand the “General Instructions for Installing SafeTCap Frame Repair Kits” before you begin.**

1. Jack up the rear of vehicle and support it on properly rated jack stands. Place rear jack stands under rear axle. Make sure the rear of vehicle is fully accessible.
2. If you are repairing both sides, **cut & repair one side at a time** keeping one side assembled as a reference/measuring point.

ART-204-R

1. Support rear axle and remove wheel.

4

****

5

Position the kit into place and roughly mark the outline. Remove kit and grind the frame down to clean metal.

Cut away the rusted area using a plasma cutter, reciprocating saw or torch.

8

******

7

6

Slide kit over frame and clamp. Tack weld kit in place. If you are installing additional kits to frame, test-fit those now to make sure they all fit together properly.

Double check all measurements and check door gaps to make sure vehicle stayed straight, then weld all edges 100% solid. If you are adding additional kits, don’t weld the ends yet.

******

Prime and paint the repaired area. Use self-tapping screws to remount any brackets that were removed.

8

**Note:** Pictures in this installation instruction sheet are for demonstration purposes only and may not actually reflect the identical make, model and year of the vehicle you are working on.